Valve KR has flow rate=17; tunnels lead to valves WA, JQ, JY, KI
Valve JN has flow rate=0; tunnels lead to valves XS, JQ
Valve JY has flow rate=0; tunnels lead to valves KR, AP
Valve WE has flow rate=0; tunnels lead to valves GY, XS
Valve HW has flow rate=0; tunnels lead to valves GP, AA
Valve QS has flow rate=0; tunnels lead to valves WW, MF
Valve MF has flow rate=15; tunnels lead to valves RJ, QS
Valve IM has flow rate=0; tunnels lead to valves WH, HS
Valve RJ has flow rate=0; tunnels lead to valves MF, PM
Valve IG has flow rate=0; tunnels lead to valves WX, ZY
Valve YL has flow rate=0; tunnels lead to valves GY, EB
Valve LI has flow rate=25; tunnels lead to valves YS, SI
Valve WW has flow rate=6; tunnels lead to valves PJ, QS
Valve QK has flow rate=0; tunnels lead to valves MV, AU
Valve AU has flow rate=20; tunnels lead to valves QK, BT, VK
Valve WH has flow rate=0; tunnels lead to valves MV, IM
Valve YS has flow rate=0; tunnels lead to valves ZL, LI
Valve FR has flow rate=0; tunnels lead to valves XS, AA
Valve NX has flow rate=0; tunnels lead to valves KI, NG
Valve OI has flow rate=5; tunnels lead to valves SU, OX, LW, JH, DK
Valve YJ has flow rate=0; tunnels lead to valves XK, XU
Valve DK has flow rate=0; tunnels lead to valves OI, IZ
Valve SU has flow rate=0; tunnels lead to valves OI, XU
Valve OH has flow rate=0; tunnels lead to valves CX, WX
Valve HS has flow rate=8; tunnels lead to valves UY, IM, WJ, XK, UC
Valve UY has flow rate=0; tunnels lead to valves HS, OX
Valve AP has flow rate=0; tunnels lead to valves JY, GY
Valve JQ has flow rate=0; tunnels lead to valves KR, JN
Valve XK has flow rate=0; tunnels lead to valves YJ, HS
Valve PM has flow rate=0; tunnels lead to valves RJ, ZY
Valve WJ has flow rate=0; tunnels lead to valves AA, HS
Valve VK has flow rate=0; tunnels lead to valves AU, SI
Valve OX has flow rate=0; tunnels lead to valves UY, OI
Valve ZL has flow rate=0; tunnels lead to valves YS, MV
Valve LW has flow rate=0; tunnels lead to valves TT, OI
Valve TT has flow rate=0; tunnels lead to valves LW, MV
Valve PJ has flow rate=0; tunnels lead to valves UC, WW
Valve UC has flow rate=0; tunnels lead to valves PJ, HS
Valve XU has flow rate=3; tunnels lead to valves EB, CW, SU, TL, YJ
Valve XS has flow rate=4; tunnels lead to valves IZ, CW, WE, JN, FR
Valve CW has flow rate=0; tunnels lead to valves XU, XS
Valve TF has flow rate=0; tunnels lead to valves AA, TL
Valve EB has flow rate=0; tunnels lead to valves XU, YL
Valve WA has flow rate=0; tunnels lead to valves KR, BT
Valve GY has flow rate=9; tunnels lead to valves GP, AP, YL, ZO, WE
Valve IZ has flow rate=0; tunnels lead to valves DK, XS
Valve KI has flow rate=0; tunnels lead to valves NX, KR
Valve AA has flow rate=0; tunnels lead to valves HW, TF, FR, JH, WJ
Valve ZO has flow rate=0; tunnels lead to valves GY, QM
Valve QM has flow rate=0; tunnels lead to valves ZO, CX
Valve SI has flow rate=0; tunnels lead to valves LI, VK
Valve BT has flow rate=0; tunnels lead to valves AU, WA
Valve BC has flow rate=0; tunnels lead to valves CX, ZY
Valve NG has flow rate=21; tunnel leads to valve NX
Valve WX has flow rate=16; tunnels lead to valves IG, OH
Valve GP has flow rate=0; tunnels lead to valves HW, GY
Valve JH has flow rate=0; tunnels lead to valves AA, OI
Valve CX has flow rate=13; tunnels lead to valves OH, BC, QM
Valve TL has flow rate=0; tunnels lead to valves TF, XU
Valve MV has flow rate=14; tunnels lead to valves QK, ZL, WH, TT
Valve ZY has flow rate=10; tunnels lead to valves PM, BC, IG
